Newsgroups: comp.sys.ibm.pc.hardware
Path: cantaloupe.srv.cs.cmu.edu!crabapple.srv.cs.cmu.edu!fs7.ece.cmu.edu!europa.eng.gtefsd.com!howland.reston.ans.net!zaphod.mps.ohio-state.edu!cs.utexas.edu!news.uta.edu!cs1442au
From: cs1442au@news.uta.edu (cs1442au)
Subject: Reboot problem
Message-ID: <1993Apr20.174559.8642@news.uta.edu>
Organization: University of Texas at Arlington
Date: Tue, 20 Apr 1993 17:45:59 GMT
Lines: 38

From x51948b1@usma1.USMA.EDU Tue Apr 20 10:28:47 1993
Received: from usma1.usma.edu by trotter.usma.edu (4.1/SMI-4.1-eef)
	id AA01628; Tue, 20 Apr 93 11:27:50 EDT
Received:  by usma1.usma.edu (5.51/25-eef)
	id AA03219; Tue, 20 Apr 93 11:20:18 EDT
Message-Id: <9304201520.AA03219@usma1.usma.edu>
Date: Tue, 20 Apr 93 11:20:17 EDT
From: x51948b1@usma1.USMA.EDU (Peckham David CDT)
To: cs1442au@decster.uta.edu
Subject: Problem.
Status: OR

--------------------

I am running a Unisys PW2 386SX20 with DOS 6.  My problem, even when I had DOS
5.0, is that when I have EMM386 loaded I can't CTL-ALT-DEL.  If I do, the
computer beeps a few times rapidly and hangs.  Then I have to use the obscure
reset (requires a screwdriver or pencil) or the power switch to reboot.  Does
anyone have a solution to this problem?

E-mail me at x51948b1@usma1.usma.edu

Dave
---------------------

Thanks,

dave
-------------------------------------------------------------------------
David S. Peckham                   |  Internet : x51948b1@usma1.usma.edu
U.S. Military Academy              |
-------------------------------------------------------------------------

-- 
 Jason Brown
cs1442au@decster.uta.edu
------------------------------------------------------------------------
Fav player Ruben Sierra
