Path: cantaloupe.srv.cs.cmu.edu!crabapple.srv.cs.cmu.edu!fs7.ece.cmu.edu!europa.eng.gtefsd.com!gatech!usenet.ins.cwru.edu!magnus.acs.ohio-state.edu!zaphod.mps.ohio-state.edu!swrinde!cs.utexas.edu!utnut!torn!newsserver.cs.uwindsor.ca!august1
From: august1@server.uwindsor.ca (AUGUSTYN  ROBERT         )
Newsgroups: comp.sys.ibm.pc.hardware
Subject: Data path width from 16 to 32 bits but speed less then double?
Message-ID: <3414@newsserver.cs.uwindsor.ca>
Date: 17 Apr 1993 23:07:27 GMT
Sender: news@server.uwindsor.ca
Organization: University of Windsor, Ontario, Canada
Lines: 5

In evolution of 80-x86 data path width has been doubled from 
8 to 16 t0 32 bits but the speed of data processing has not increased at
same rate.The question is Why? What is relationship bettween data path width and data processing speed?
Thanks in advance for the input.
Robert. 
