Newsgroups: comp.sys.ibm.pc.hardware
Path: cantaloupe.srv.cs.cmu.edu!crabapple.srv.cs.cmu.edu!bb3.andrew.cmu.edu!news.sei.cmu.edu!cis.ohio-state.edu!zaphod.mps.ohio-state.edu!usc!elroy.jpl.nasa.gov!ames!amdcad!dvorak.amd.com!tdbear
From: tdbear@dvorak.amd.com (Tom Barrett)
Subject: Re: The "P24T"
Message-ID: <1993Apr21.132101.21973@dvorak.amd.com>
Organization: Advanced Micro Devices, Inc.; Austin, Texas
References: <1r29td$17r@usenet.INS.CWRU.Edu>
Date: Wed, 21 Apr 93 13:21:01 GMT
Lines: 16

In article <1r29td$17r@usenet.INS.CWRU.Edu> rrn@po.CWRU.Edu (Robert R. Novitskey) writes:
>    Has anyone out there heard of any performance stats on the fabled p24t.
> I was wondering what it's performance compared to the 486/66 and/or
>pentium would be.  Any info would be helpful.

An advertisement in MicroTimes (a bay area mini-Computer Shopper) from
ENCY systems in Fremont has a graphic for the P24T performance based
on MIPS (power meter v1.7):  the 486DX-33 raked in about 14-15, the 
486DX2-66 got about 24, and the P24T-66 got about 44-45.

Tom
-- 
|Tom Barrett (TDBear), Sr. Engineer|tom.barrett@amd.com|v:512-462-6856 |
|AMD PCD MS-520 | 5900 E. Ben White|Austin, TX  78741  |f:512-462-5155 |
|...don't take no/take hold/don't leave it to chance ---Tasmin Archer  |
|My views are my own and may not be the same as the company of origin  |
