Newsgroups: comp.sys.ibm.pc.hardware
Path: cantaloupe.srv.cs.cmu.edu!rochester!udel!gatech!howland.reston.ans.net!zaphod.mps.ohio-state.edu!caen!batcomputer!munnari.oz.au!newshost.anu.edu.au!csc.canberra.edu.au!kari!tp924353
From: tp924353@kari.canberra.edu.au (Jason Wolfgang Hecker)
Subject: Problems with parallel I/O.
Message-ID: <tp924353.735532017@kari>
Sender: news@csc.canberra.edu.au
Organization: Info Sci & Eng, University of Canberra, AUSTRALIA
Date: 23 Apr 93 02:26:57 GMT
Lines: 9

I writing a program that uses the parallel port. My problem is that I need to
generate an interrupt when the ack line is pulsed. I can get this to occur  
once, but am unable to generate succesive interrupts.

Can someone suggest how I may resolve this problem.

Thanks.


