Newsgroups: comp.graphics
Path: cantaloupe.srv.cs.cmu.edu!magnesium.club.cc.cmu.edu!news.sei.cmu.edu!cis.ohio-state.edu!zaphod.mps.ohio-state.edu!cs.utexas.edu!uunet!comp.vuw.ac.nz!cc-server4.massey.ac.nz!ARowatt
From: ARowatt@massey.ac.nz (A.J. Rowatt)
Subject: Page flipping in VGA 320x200x256 mode.
Message-ID: <1993Apr19.204616.16511@massey.ac.nz>
Organization: Massey University, Palmerston North, New Zealand
X-Reader: NETNEWS/PC Version 2c
Date: Mon, 19 Apr 93 20:46:16 GMT
Lines: 12

Help!
How do you write to the second bank/page of memory when in VGA
320x200x256 colour mode?. ie: to perform page flipping animation
and buffering of the screen.
     I have tried using the Map Mask Registers, but this does not
perform the required task (Although it does do something).

Note: It *must* be able to work on a standard VGA (ie: not
necessarily a SVGA card).

Many thanx in advance...
Andrew
