Xref: cantaloupe.srv.cs.cmu.edu rec.autos:103007 rec.autos.tech:54109 sci.materials:1689
Newsgroups: rec.autos,rec.autos.tech,sci.materials
Path: cantaloupe.srv.cs.cmu.edu!das-news.harvard.edu!noc.near.net!howland.reston.ans.net!darwin.sura.net!convex!tobias
From: tobias@convex.com (Allen Tobias)
Subject: Re: Auto air conditioning without Freon
Message-ID: <1993Apr22.195519.11104@convex.com>
Sender: usenet@convex.com (news access account)
Nntp-Posting-Host: hydra.convex.com
Organization: CONVEX Computer Corporation, Richardson, Tx., USA
References: <20APR199313375138@erich.triumf.ca> <1993Apr21.034751.23512@ntuix.ntu.ac.sg> <C5u5Fy.Hvx@news.cso.uiuc.edu>
Distribution: usa
Date: Thu, 22 Apr 1993 19:55:19 GMT
X-Disclaimer: This message was written by a user at CONVEX Computer
              Corp. The opinions expressed are those of the user and
              not necessarily those of CONVEX.
Lines: 16

In article <C5u5Fy.Hvx@news.cso.uiuc.edu> tspila@uxa.cso.uiuc.edu (Tim Spila {Romulan}) writes:
>In article <1993Apr21.034751.23512@ntuix.ntu.ac.sg> mgqlu@ntuix.ntu.ac.sg (Max Lu) writes:
>>We are working on gas-solid adsorption air-con system for auto applications.
>>In this kind of system, the energy for regenerating the adsorbent is from 
>>the exhaust gas.  Anyone interested in this mail email me or follow up this
>>thread, we may have a discussion on prospects of this technology.
>
>Ok, I'll bite.  How is this supposed to work?
>
>Tim.

Better still, years ago they demonstrated a cold air system which only used
"air". It was called a Rovax. The unit worked very well, the short coming
was the seal technology. Where is it today?

AT
