Newsgroups: rec.motorcycles
Path: cantaloupe.srv.cs.cmu.edu!das-news.harvard.edu!noc.near.net!uunet!pipex!sunic!uts!daimi!jbuhl
From: jbuhl@daimi.aau.dk (Jesper Buhl)
Subject: Re: VFR + ST11 Owners get hidden feature
Message-ID: <1993Apr26.080848.3443@daimi.aau.dk>
Keywords: lights
Sender: news@daimi.aau.dk
Organization: DAIMI: Computer Science Department, Aarhus University, Denmark
References: <C61r0B.C7@world.std.com> <1993Apr25.211819.4730@linus.mitre.org>
Date: Mon, 26 Apr 93 08:08:48 GMT
Lines: 22

cookson@mbunix.mitre.org (Cookson) writes:

>In article <C61r0B.C7@world.std.com> daved@world.std.com (Dave T Dorfman) writes:
>> I was enjoying lunch this saturday at foodies in Milford NH with an assortment
>>of other nedod folks when Dean Cookson ( yes he has not left the 
>>country, yet) mentioned that the wiring diagram of the VFR750 
>>shows that  the light switch is a three position switch. 
>>
>My CB750 does it too.  The "Switch Continuity" section of the wiring diagram
>looks something like this:

>	HL L  H
>        x--x     Low
>        x--x--x  (N)
>        x-----x  High

And my '78 CX500 too - I first thought it was the wiring diagram that didn't
fit MY machine ;-)

>Dean

/jb
