Xref: cantaloupe.srv.cs.cmu.edu rec.autos:102986 rec.autos.tech:54092 sci.materials:1680
Newsgroups: rec.autos,rec.autos.tech,sci.materials
Path: cantaloupe.srv.cs.cmu.edu!magnesium.club.cc.cmu.edu!news.sei.cmu.edu!cis.ohio-state.edu!zaphod.mps.ohio-state.edu!sdd.hp.com!ux1.cso.uiuc.edu!news.cso.uiuc.edu!uxa.cso.uiuc.edu!tspila
From: tspila@uxa.cso.uiuc.edu (Tim Spila {Romulan})
Subject: Re: Auto air conditioning without Freon
Date: Wed, 21 Apr 1993 13:28:45 GMT
Message-ID: <C5u5Fy.Hvx@news.cso.uiuc.edu>
Distribution: usa
References: <20APR199313375138@erich.triumf.ca> <1993Apr21.034751.23512@ntuix.ntu.ac.sg>
Sender: usenet@news.cso.uiuc.edu (Net Noise owner)
Organization: University of Illinois at Urbana
Lines: 9

In article <1993Apr21.034751.23512@ntuix.ntu.ac.sg> mgqlu@ntuix.ntu.ac.sg (Max Lu) writes:
>We are working on gas-solid adsorption air-con system for auto applications.
>In this kind of system, the energy for regenerating the adsorbent is from 
>the exhaust gas.  Anyone interested in this mail email me or follow up this
>thread, we may have a discussion on prospects of this technology.

Ok, I'll bite.  How is this supposed to work?

Tim.
