Newsgroups: comp.sys.ibm.pc.hardware
Path: cantaloupe.srv.cs.cmu.edu!rochester!udel!gatech!usenet.ufl.edu!usenet.cis.ufl.edu!caen!batcomputer!lynx@msc.cornell.edu!news
From: randy@msc.cornell.edu
Subject: SCSI vs. IDE
Message-ID: <1993Apr13.134711.25857@msc.cornell.edu>
Sender: news@msc.cornell.edu
Organization: Cornell University
Date: Tue, 13 Apr 1993 13:47:11 GMT
Lines: 8

Do all SCSI cards for DOS systems require a separate device driver to be loaded
into memory for each SCSI device hooked up?  Will this also be true of the 32-bit
OS's?

Thanks.

Randy

