Newsgroups: rec.motorcycles
Path: cantaloupe.srv.cs.cmu.edu!das-news.harvard.edu!noc.near.net!howland.reston.ans.net!usc!elroy.jpl.nasa.gov!lll-winken.llnl.gov!myrddin!seahunt.imat.com!nelson
From: nelson@seahunt.imat.com (Michael Nelson)
Subject: Re: Need Maintenance tips
Message-ID: <C5uDs9.DoG@myrddin.imat.com>
Sender: usenet@myrddin.imat.com (Da News)
Nntp-Posting-Host: seahunt.imat.com
Organization: SeaHunt, San Francisco CA
References: <C5rIwA.2or@world.std.com>
Date: Wed, 21 Apr 1993 16:28:54 GMT
Lines: 20

In article <C5rIwA.2or@world.std.com> CGKarras@world.std.com (Christopher G Karras) writes:
>
>After reading the service manual for my bike (Suzuki GS500E--1990) I have
>a couple of questions I hope you can answer:
>
>When checking the oil level with the dip stick built into the oil fill
>cap, does one check it with the cap screwed in or not?

	Most bikes I've seen that use a dipstick rather than a
	sight glass are designed to check it without screwing it
	in.  In the manual for my CBR900RR, they specifically
	state it should be done this way.

				Michael

-- 
+-------------------------------------------------------------+
| Michael Nelson                                1993 CBR900RR |
| Internet: nelson@seahunt.imat.com                 Dod #0735 |
+-------------------------------------------------------------+
