Xref: cantaloupe.srv.cs.cmu.edu comp.os.ms-windows.misc:9751 comp.os.ms-windows.apps:11809
Newsgroups: comp.os.ms-windows.misc,comp.os.ms-windows.apps
Path: cantaloupe.srv.cs.cmu.edu!crabapple.srv.cs.cmu.edu!fs7.ece.cmu.edu!europa.eng.gtefsd.com!howland.reston.ans.net!noc.near.net!uunet!comp.vuw.ac.nz!ferrari.datamark.co.nz!thomas
From: thomas@datamark.co.nz (Thomas Beagle)
Subject: Re: WINQVTNET with NDIS on Token Ring ?
Message-ID: <1993Apr21.210954.40516@datamark.co.nz>
Date: Wed, 21 Apr 1993 21:09:54 GMT
References: <1993Apr21.082152@liris.tew.kuleuven.ac.be>
Organization: Datamark International Ltd.
Lines: 14

In article <1993Apr21.082152@liris.tew.kuleuven.ac.be> wimvh@liris.tew.kuleuven.ac.be (Wim Van Holder) writes:
>Is it possible to use WinQVT/Net on a machine that uses NDIS to connect to a
>Token Ring ? I tried it with older versions (< 3.2) but got an invalid packet
>class error or something the like...

How are you attempting to do that?

Are you using the DIS_PKT9 program? This provides a packet driver on
top of the NDIS driver.

-- 
   Thomas Beagle | thomas@datamark.co.nz        Work: 64 4 233 8186    __o
Technical Writer | thomas@cavebbs.welly.gen.nz  Home: 64 4 499 3832  _-\<,
  Wellington, NZ |    Hound for hire. Will work for dog biscuits.   (_)/(_)
