Newsgroups: comp.sys.ibm.pc.hardware
Path: cantaloupe.srv.cs.cmu.edu!crabapple.srv.cs.cmu.edu!bb3.andrew.cmu.edu!news.sei.cmu.edu!fs7.ece.cmu.edu!europa.eng.gtefsd.com!howland.reston.ans.net!agate!ames!data.nas.nasa.gov!binky.nas.nasa.gov!butzen
From: butzen@binky.nas.nasa.gov (Nicholas A. Butzen)
Subject: Re: GW2000 and SIMMS
References: <113956@bu.edu> <1pq2ofINNe2t@darkstar.UCSC.EDU>
Sender: news@nas.nasa.gov (News Administrator)
Organization: NAS Program, NASA Ames Research Center, Moffett Field, CA
Date: Mon, 5 Apr 93 21:16:22 GMT
Message-ID: <1993Apr5.211622.28288@nas.nasa.gov>
Lines: 29

They are actually 72 pin. They come in 4, 8, 16, and 32 with 64s soon
If you are interested in 4s or 8s, I may be able to help. Please call
415-324-2881 after 4:00 pm pdt. I may be interested in a trade.



				NAB
				ASAN-NASA it's all done with mirrors
In article <1pq2ofINNe2t@darkstar.UCSC.EDU>, banshee@cats.ucsc.edu (Wailer at the Gates of Dawn) writes:
|> 
|> In <113956@bu.edu> nshah@acs2.bu.edu writes:
|> 
|> >I have a gateway2000 483/33 local bus system.  It has 4 slots for SIMMS
|> >that either have to use 4 or 16MB simms.  My question:  I just
|> >received a 4x9 70ns simm and it has ~30 pins.  The slot on the
|> >motherboard has at least 70 or so pins.  Did I get the wrong simm
|> >or can I still use my simm , although not all the pins on the slot would
|> >be flilled.  I have never encountered such a long slot for simms before.
|> >Anyone have suggestions?  I can't get a hold of Gateway yet.  Thanks
|> >Please post to the net or :   nshah@acs.bu.edu
|> 
|> Yes you got the wrong simm.  You need 70 pin simms in 4 or 16 meg
|> flavors.
|> 
|> -- 
|> The Wailer at the Gates of Dawn              | banshee@cats.UCSC.EDU       |
|> Just who ARE you calling a FROOFROO Head?    |                             |
|> DoD#0667  "Just a friend of the beast."      | banshee@ucscb.UCSC.EDU      |
|> 2,3,5,7,13,17,19,31,61,89,107,127,521,607....| banshee@ucscb.BITNET        |
