Path: cantaloupe.srv.cs.cmu.edu!magnesium.club.cc.cmu.edu!news.sei.cmu.edu!cis.ohio-state.edu!zaphod.mps.ohio-state.edu!usc!sol.ctr.columbia.edu!destroyer!cs.ubc.ca!mala.bc.ca!apland
From: apland@mala.bc.ca (Ron Apland)
Newsgroups: comp.os.ms-windows.misc
Subject: Re: W4WG & Novell
Message-ID: <1993Apr26.211308.1733@mala.bc.ca>
Date: 26 Apr 93 21:13:08 -0700
References: <1rh2mi$ea4@msuinfo.cl.msu.edu> <1993Apr27.102626.1@csc.canterbury.ac.nz>
Organization: Malaspina College
Lines: 29

In article <1993Apr27.102626.1@csc.canterbury.ac.nz>, cctr132@csc.canterbury.ac.nz (Nick FitzGerald, PC Software Consultant, CSC, UoC, NZ) writes:
> In article <1rh2mi$ea4@msuinfo.cl.msu.edu>, bilan@cps.msu.edu (Thomas J
> Bilan) writes:
> 
>> If I put LASTDRIVE = Z in my config.sys, NETX will run but I can't access
>> drive f: to log in to Novell.  
>> If I don't put LASTDRIVE = Z in my config.sys I can't access other W4WG 
>> drives from the file-manager.
>>
>> It seems that there should be a way to make NETX work with the LASTDRIVE = 
>> statement in my Config.Sys.
> 
> First off, I haven't used W4WG (but I think that's about to change!).
> 
> The problem is the LASTDRIVE command and the way NetWare in general (and
> in this case NETX in particular) adds drives to the device chain. 
> Setting LASTDRIVE=Z means there are no "unassigned" (as opposed to
> "unused") drive letters for NetWare to use, as it tacks its drive
> mappings -onto the end- of the existing list of drives.  W4WG obviously
> attaches its network drives to "existing, unused" drive letters.
> 
> I'd guess the next thing I'd try is something like LASTDRIVE=M, which on
> most machines will leave a fair swathe of drives for W4WG and still
> allow up to 13 NetWare drive mappings as well.

W4WG requires DOS drives.  I use LASTDRIVE=J which makes my first Novell drive
K and leaves me drives G, H, I and J for W4WG.  My local DOS drives use A-F.

Ron
