Newsgroups: comp.sys.ibm.pc.hardware
Path: cantaloupe.srv.cs.cmu.edu!das-news.harvard.edu!noc.near.net!howland.reston.ans.net!usc!elroy.jpl.nasa.gov!ames!news.Hawaii.Edu!iniki!himb
From: himb@iniki.soest.hawaii.edu (Liz Camarra)
Subject: Some more info. about P9000 board
Message-ID: <C5pHE7.JtK@news.Hawaii.Edu>
Originator: himb@iniki
Sender: news@news.Hawaii.Edu
Organization: School of Ocean and Earth Science and Technology
Date: Mon, 19 Apr 1993 00:58:55 GMT
Lines: 10

  One more thing to add, the Orchid board vesa bios is only
able to handle the 1 meg dram on board, the Viper however can
utilize the 2 meg vram on board to support vesa modes such as
1280x1024x256, 800x600x16 mil. and 1024x768x65536 under Dos.

+----------------------------------------------------------------+
Stephen Lau, Elec. Engineering, Univ. of Hawaii
 don't have my own account until grad. school starts (autumn 93)
+              Death to FM synthesis! Go Gus!                    +

