Xref: cantaloupe.srv.cs.cmu.edu comp.unix.dos-under-unix:443 comp.sys.ibm.pc.misc:34162 comp.os.ms-windows.apps:11609 comp.os.ms-windows.misc:9582 alt.uu.comp.os.linux.questions:209 comp.apps.spreadsheets:1154 comp.misc:20374 alt.os.linux:2912 comp.os.linux:37143
Newsgroups: comp.unix.dos-under-unix,comp.sys.ibm.pc.misc,comp.sys.ibm.pc.net,comp.os.ms-windows.apps,comp.os.ms-windows.misc,alt.uu.comp.os.linux.questions,comp.apps.spreadsheets,comp.misc,alt.os.linux,comp.os.linux,man.linux
Path: cantaloupe.srv.cs.cmu.edu!das-news.harvard.edu!noc.near.net!howland.reston.ans.net!newsserver.jvnc.net!news.edu.tw!netcentral.tit.edu.tw!news!news.csie.nctu.edu.tw!ghhwang
From: ghhwang@csie.nctu.edu.tw (ghhwang)
Subject: Re: WP-PCF, Linux, RISC?
Message-ID: <C5o1yq.M34@csie.nctu.edu.tw>
Sender: usenet@csie.nctu.edu.tw
Organization: Computer Sci. & Information Eng., Chiao-Tung U, Taiwan, ROC
X-Newsreader: TIN [version 1.1 PL6]
References: <C56HEo.KKA@ccu.umanitoba.ca>
Date: Sun, 18 Apr 1993 06:28:02 GMT
Lines: 7

Dear friend,
  The RISC means "reduced instruction set computer". The RISC usually has 
small instruction set so as to reduce the circuit complex and can increase 
the clock rate to have a high performance. You can read some books about
computer architecture for more information about RISC.
                       
                                   ghhwang@csie.nctu.edu.tw form R.O.C TaiwaN 
