Path: cantaloupe.srv.cs.cmu.edu!crabapple.srv.cs.cmu.edu!fs7.ece.cmu.edu!europa.eng.gtefsd.com!gatech!swrinde!zaphod.mps.ohio-state.edu!darwin.sura.net!haven.umd.edu!uunet!pipex!uknet!uknet!edcastle!cam
From: cam@castle.ed.ac.uk (Chris Malcolm)
Newsgroups: sci.electronics
Subject: CASIO SF7500 SERIAL LINK
Message-ID: <34325@castle.ed.ac.uk>
Date: 16 Apr 93 15:19:28 GMT
Organization: Edinburgh University
Lines: 8

The Casio 7500 lectric diary has a 3-wire serial interface with param
setting like RS232, for which one get a magic but expensive cable to
connect to a PC. Does anyone know the spec of this interface, e.g., it
needs inverting and boosting from CMOS signals to match RS232 lines?
-- 
Chris Malcolm    cam@uk.ac.ed.aifh          +44 (0)31 650 3085
Department of Artificial Intelligence,    Edinburgh University
5 Forrest Hill, Edinburgh, EH1 2QL, UK                DoD #205
